**User Manual**

User needs to connect the instrument to the PC or Laptop via USB.

User needs to install arduino 1.0.4.

User needs arduino uno and arduino Ethernet shield.

User needs to place the sensor under his/her armpit or behind the earlobe.

1. Start arduino.
2. Compile the temperature.ino file.
3. Upload it on arduino board.
4. Check the serial monitor for the output.
5. Login to the website
6. Go to the facilities section
7. The temperature will be displayed.